,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##,Mat##OTHER##,SEO##OTHER##
Taro 3P SRS-MF LED3000-830 A35 01,0.14,0.14,0.145,10121357,6384940,Verkehrsweiß RAL 9016,1.535,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6384940,Schutzklasse I,IP20,ET,LED,31,80,2701,3000,Taro_LS : TX042116,TRILUX_Alu_RAL_9016,TRILUX_3000_Taro
Taro 3P SRS-MF LED3000-840 A37 01,0.14,0.14,0.145,10121358,6385040,Verkehrsweiß RAL 9016,1.535,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6385040,Schutzklasse I,IP20,ET,LED,31,80,2895,4000,Taro_LS : TX042117,TRILUX_Alu_RAL_9016,TRILUX_4000_Taro
Taro 3P SRS-MF LED4000-830 A39 01,0.14,0.14,0.145,10121362,6385440,Verkehrsweiß RAL 9016,1.535,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6385440,Schutzklasse I,IP20,ET,LED,39,80,3450,3000,Taro_LS : TX042118,TRILUX_Alu_RAL_9016,TRILUX_3000_Taro
Taro 3P SRS-MF LED4000-840 A41 01,0.14,0.14,0.145,10121361,6385340,Verkehrsweiß RAL 9016,1.535,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6385340,Schutzklasse I,IP20,ET,LED,39,80,3640,4000,Taro_LS : TX042119,TRILUX_Alu_RAL_9016,TRILUX_4000_Taro
Taro 3P SRS-SP LED4000-830 A10 01,0.14,0.14,0.145,10121359,6385140,Verkehrsweiß RAL 9016,1.535,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6385140,Schutzklasse I,IP20,ET,LED,39,80,3448,3000,Taro_LS : TX042120,TRILUX_Alu_RAL_9016,TRILUX_3000_Taro
Taro 3P SRS-SP LED4000-840 A41 01,0.14,0.14,0.145,10121360,6385240,Verkehrsweiß RAL 9016,1.535,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6385240,Schutzklasse I,IP20,ET,LED,39,80,3638,4000,Taro_LS : TX042121,TRILUX_Alu_RAL_9016,TRILUX_4000_Taro
