,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##,Mat##OTHER##,SEO##OTHER##
TaroEB SRS-MF LED3000-830 A35 ET 01,0.14,0.14,0.145,10121373,6386750,Verkehrsweiß RAL 9016,1.065,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6386750,Schutzklasse I,IP20,ET,LED,31,80,2701,3000,Taro_LS : TX042122,TRILUX_Alu_RAL_9016,TRILUX_3000_Taro
TaroEB SRS-MF LED3000-840 A37 ET 01,0.14,0.14,0.145,10121374,6386850,Verkehrsweiß RAL 9016,1.065,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6386850,Schutzklasse I,IP20,ET,LED,31,80,2895,4000,Taro_LS : TX042123,TRILUX_Alu_RAL_9016,TRILUX_4000_Taro
