,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##,Mat##OTHER##,SEO##OTHER##
TaroMiniEB SRS-MF LED3000-830 A02 E 01,0.093,0.093,0.11,10121375,6386950,Verkehrsweiß RAL 9016,1.065,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6386950,Schutzklasse I,IP20,ET,LED,33,80,2744,3000,Taro_LS : TX042126,TRILUX_Alu_RAL_9016,TRILUX_3000_Taro
TaroMiniEB SRS-MF LED3000-840 A33 ET 01,0.093,0.093,0.11,10121376,6387050,Verkehrsweiß RAL 9016,1.065,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6387050,Schutzklasse I,IP20,ET,LED,33,80,2942,4000,Taro_LS : TX042115,TRILUX_Alu_RAL_9016,TRILUX_4000_Taro
