,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##,Mat##OTHER##,SEO##OTHER##
"TaroPL 3PH9 FL LED3000-830 A06 L1,5 01",0.14,0.14,0.145,10121393,6388740,TaroPL_GH : 3PH9,Verkehrsweiß RAL 9016,2.2,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6388740,Schutzklasse I,IP20,ET,LED,31,80,2779,3000,Taro_LS : TX042127,TRILUX_Alu_RAL_9016,TRILUX_3000_Taro
"TaroPL 3PH9 FL LED3000-840 A37 L1,5 01",0.14,0.14,0.145,10121394,6388840,TaroPL_GH : 3PH9,Verkehrsweiß RAL 9016,2.2,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6388840,Schutzklasse I,IP20,ET,LED,31,80,2979,4000,Taro_LS : TX042128,TRILUX_Alu_RAL_9016,TRILUX_4000_Taro
"TaroPL H9 FL LED3000-830 A35 L1,5 01",0.14,0.14,0.145,10121395,6388940,TaroPL_GH : H9,Verkehrsweiß RAL 9016,2.2,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6388940,Schutzklasse I,IP20,ET,LED,31,80,2779,3000,Taro_LS : TX042129,TRILUX_Alu_RAL_9016,TRILUX_3000_Taro
"TaroPL H9 FL LED3000-840 A37 L1,5 01",0.14,0.14,0.145,10121396,6389040,TaroPL_GH : H9,Verkehrsweiß RAL 9016,2.2,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6389040,Schutzklasse I,IP20,ET,LED,31,80,2979,4000,Taro_LS : TX042130,TRILUX_Alu_RAL_9016,TRILUX_4000_Taro
